|  |  |  |
| --- | --- | --- |
| Positives for House Building | Material/Key Properties | Negatives for House Building |
|  | **Wood** C:\Users\cmackinnon\AppData\Local\Temp\d34824fb-c46f-4cc1-88e1-4570dee5d0cd.pngstrong, rigid, quite flammable, opaque |  |
|  | **Straw**C:\Users\cmackinnon\AppData\Local\Temp\b821a18b-3657-4933-9d95-f7a168df86a8.pngfragile, flexible, very flammable, opaque  |  |
|  | **Pitch**C:\Users\cmackinnon\AppData\Local\Temp\42f5ba47-636c-4f43-816d-6ff7150d0197.pngflexible, waterproof, extremely flammable, opaque |  |
|  | **Glass**C:\Users\cmackinnon\AppData\Local\Temp\9f674fd2-497e-4d5c-96f9-0783f7ee01a0.pngfragile, rigid, transparent |  |